## Specs of the Lathe

The specifications of the Colchester 1800 Lathe

The Motor was capable of reaching 2.2kW (3 h.p) which was directed by a twin V-Belt gear set up. Which was also 3 phase as well.

Swing Over: Bed 342mm, Cross Slide 215mm, Gap 480mm

Distance Between Centres: 609mm

Floor Plan / Foot Print: 1.7m x 1.15m

Weight: 0.79 Tons Approx.

Equipped with: 3 & 4 Jaw Chucks, Low Volt Light, Imperial/Metric threading and coolant & chuck guard.